# 2023 Ram Commercial 3500, 4500 & 5500 Chassis Cab

## FEATURE AVAILABILITY

S = Standard. O = Optional. P = Part of package. NA = Not available.   
Note: some features and/or applications may be late availability.

### CONFIGURATION

#### 3500 – Body Model

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3500 – Body Model | TRADESMAN | SLT | LARAMIE | LIMITED |
| Regular Cab — 60-in. CA (143.5-in. wheelbase) | S | S | NA | NA |
| Regular Cab — 84-in. CA (167.5-in. wheelbase) (N/A with 10,000-lb. GVWR) | S | S | NA | NA |
| Crew Cab — 60-in. CA (172.4-in. wheelbase) | O | O | S | S |

#### 3500 – Drive System

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 3500 – Drive System | TRADESMAN | SLT | LARAMIE | LIMITED |
| 4x2 | S | S | S | S |
| 4x4 | O | O | O | O |

#### 4500/5500 – Body Model

| 4500/5500 – Body Model | TRADESMAN | SLT | LARAMIE | LIMITED |
| --- | --- | --- | --- | --- |
| Regular Cab — 60-in. CA (144.5-in. wheelbase) | S | S | NA | NA |
| Regular Cab — 84-in. CA (168.5-in. wheelbase) | S | S | NA | NA |
| Regular Cab — 108-in. CA (192.5-in. wheelbase) | S | S | NA | NA |
| Regular Cab — 120-in. CA (204.5-in. wheelbase) | S | S | NA | NA |
| Crew Cab — 60-in. CA (173.5-in. wheelbase) | O | O | S | S |
| Crew Cab — 84-in. CA (197.4-in. wheelbase) | O | O | S | S |

#### 4500/5500 – Drive System

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4500/5500 – Drive System | TRADESMAN | SLT | LARAMIE | LIMITED |
| 4x2 | S | S | S | S |
| 4x4 | O | O | O | O |

### POWERTRAIN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Engine / Transmission | TRADESMAN | SLT | LARAMIE | LIMITED |
| 6.4-liter HEMI® V-8 (3500) with eight-speed 8HP75 automatic transmission | S | S | S | S |
| 6.4-liter HEMI V-8 (3500/4500/5500) with six-speed AS66RC  Aisin automatic transmission | S/P | S/P | S/P | S/P |
| 6.7-liter Cummins Turbo Diesel I-6 engine with six-speed AS69RC  Aisin automatic transmission | O | O | O | O |

### MECHANICAL

| Alternator | TRADESMAN | SLT | LARAMIE | LIMITED |
| --- | --- | --- | --- | --- |
| 180-amp | S | S | S | S |
| 220-amp (Included on 3500/4500/5500 models with Heavy-Duty  Snowplow Prep Group; included with Electrical Accessory Group  and Ambulance Prep Group) | O/P | O/P | O/P | O/P |
| 380-amp (dual 160-amp and 220-amp; requires 6.4-liter) | O | O | O | O |
| 440-amp (dual 220-amp alternators; requires 6.7-liter) | O/P | O/P | O/P | O/P |

#### Axles: 3500

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Axles: 3500 | TRADESMAN | SLT | LARAMIE | LIMITED |
| Single Rear Wheel Group | S | S | S | S |
| Dual rear wheels | O | O | O | O |
| Front, 6,000-lb. GAWR (SRW axle) | S | S | S | S |
| Rear, 11.50-in. (SRW axle) | S | S | S | S |
| Front, 205 mm (DRW axle) | S/O | S/O | S/O | S/O |
| Rear, 11.50-in. (DRW axle) | S/O | S/O | S/O | S/O |
| Rear, 12.0-in. (DRW axle) | P | P | P | P |

#### Axle Ratios: 3500

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Axle Ratios: 3500 | TRADESMAN | SLT | LARAMIE | LIMITED |
| 3.73 ratio (packaged with diesel models only) | P | P | P | P |
| 4.10 ratio (standard with gas) | S | S | S | S |
| Rear, anti-spin differential | S | S | S | S |

#### Axles: 4500/5500

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Axles: 4500/5500 | TRADESMAN | SLT | LARAMIE | LIMITED |
| Dual rear wheel | S | S | S | S |
| Front, 10.5-in. | S | S | S | S |
| Front, 10.5-in., 7,250-lb. GAWR | O | O | O | O |
| Front-axle disconnect (4500/5500 4x4) | S | S | S | S |
| Rear, anti-spin differential | S | S | S | S |

#### Axle Ratios:4500

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Axle Ratios: 4500 | TRADESMAN | SLT | LARAMIE | LIMITED |
| Rear, 4.10 ratio (packaged with 4500 with 6.7-liter engine) | P | P | P | P |
| 4.44 ratio | S | S | S | S |
| 4.89 ratio (available with 6.4-liter engine) | O/P | O/P | O/P | O/P |
| Rear, American Axle (12,000-lb. GAWR) | S | S | S | S |

#### Axle Ratios: 5500

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Axle Ratios: 5500 | TRADESMAN | SLT | LARAMIE | LIMITED |
| 4.44 ratio | S | S | S | S |
| 4.89 ratio | O/P | O/P | O/P | O/P |
| Rear, American Axle, (13,500-lb. GAWR) | S | S | S | S |

#### Fuel Tank

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Fuel Tank | TRADESMAN | SLT | LARAMIE | LIMITED |
| 52-gallon, rear | S | S | S | S |
| 74-gallon dual fuel tanks (52 and 22 gals.) | O | O | O | O |
| 22-gallon mid-ship fuel tank | O | O | O | O |

#### Power Take Off (PTO)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Power Take Off (PTO) | TRADESMAN | SLT | LARAMIE | LIMITED |
| Stationary elevated engine idle up | S | S | S | S |
| Right-side PTO | O | O | O | O |
| Left-side PTO | O | O | O | O |
| Split-shaft PTO (packaged with PTO, if diesel) | P | P | P | P |
| Hard-wired remote start/stop (packaged with PTO) | P | P | P | P |

### EXTERIOR

#### Engine Shut-Off Timer

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Engine Shut-Off Timer | TRADESMAN | SLT | LARAMIE | LIMITED |
| 6.4-liter and 6.7-liter (5 minutes) (dealer programmable from 1 to 60 minutes) | O | O | O | O |

### INTERIOR

#### Instrument Cluster Displays

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Instrument Cluster Displays | TRADESMAN | SLT | LARAMIE | LIMITED |
| Cluster 3.5-in. thin-film transistor (TFT) black  and white display | S | S | NA | NA |
| Cluster 3.5-in. TFT color display | NA | P | NA | NA |
| Cluster 7.0-in. TFT color display | P | P | S | S |

#### Telematics

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Telematics | TRADESMAN | SLT | LARAMIE | LIMITED |
| Ram Telematics System by Telogis | O | O | O | O |

#### Upfitter Interface

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Upfitter Interface | TRADESMAN | SLT | LARAMIE | LIMITED |
| Vehicle system interface module (VSIM) | S | S | S | S |

### UCONNECT MULTIMEDIA

#### Bluetooth

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Bluetooth | TRADESMAN | SLT | LARAMIE | LIMITED |
| Uconnect Voice Command with Bluetooth | S | S | S | S |

#### Compass

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Compass | TRADESMAN | SLT | LARAMIE | LIMITED |
| Compass display in the radio (Tradesman availability only with optional  5.0-in. radio) | P | S | S | S |
| GPS antenna input on radio (packaged with 5.0-in., 8.4-in. and 12.0-in. radios) | P | P | P | P |

#### Connectivity

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Connectivity | TRADESMAN | SLT | LARAMIE | LIMITED |
| Front: Media hub — includes two fully functional type A/C USB port pairs  and one auxiliary jack (four USB connection points) | S | S | S | S |
| Middle: 2.5-amp charge only single USB port (located in center console  or armrest) | S | S | S | S |
| Rear: Dual remote USB port 2 A/C pairs; one pair fully functional, one pair charge only (packaged with Luxury Group) | NA | P | S | S |
| Auxiliary headphone jack for mobile devices | S | S | S | S |
| Wireless charging pad (includes CD player; packaged with Laramie) | NA | NA | P | S |

#### Power

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Power | TRADESMAN | SLT | LARAMIE | LIMITED |
| Accessory delay | S | S | S | S |
| Auxiliary outlets (one battery and one ignition-fed) | S | S | S | S |
| 115-volt auxiliary power outlet, instrument panel-mounted (Tradesman option)  (packaged with SLT) | O | P | S | S |
| 115-volt auxiliary power outlet, rear facing, (Crew Cab only)  (packaged with SLT) | NA | P | S | S |
| 400-watt inverter | P | P | P | P |

#### Radios

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Radios | TRADESMAN | SLT | LARAMIE | LIMITED |
| Uconnect 3.0 (hands-free Bluetooth), associated display | S | NA | NA | NA |
| Uconnect 5.0 — AM/FM with 5.0-in. touchscreen display, media hub  (USB, Auxiliary), Bluetooth, SiriusXM Radio, associated display | O | S | NA | NA |
| Uconnect 8.4 — AM/FM with 8.4-in. touchscreen display, media hub (USB, Auxiliary), Uconnect with Bluetooth, SiriusXM Radio, HD radio, associated display | NA | O | S | NA |
| Uconnect 8.4 AM/FM with 8.4-in. touchscreen display, media hub (USB, Auxiliary),  Navigation, Uconnect with Bluetooth, SiriusXM Radio, HD radio, (packaged with Laramie) (SLT option is Crew only) | NA | O | O/P | S |
| Uconnect 12.0 — AM/FM/BT/SiriusXM Radio/NAV/HD/CELL, Apple CarPlay and Android Auto, SiriusXM Radio (packaged with Limited) | NA | NA | O | O/P |
| Radio controls, steering wheel-mounted audio controls | P | P | S | S |

### SAFETY AND SECURITY

#### Camera

| Camera | TRADESMAN | SLT | LARAMIE | LIMITED |
| --- | --- | --- | --- | --- |
| ParkView rear backup camera | O | O | O | S |
| Cargo View camera requires 8.4-in. or 12-in. radio, includes LED CHMSL  and cargo lamps | NA | O | O | O |
| Auxiliary remote camera (Mopar camera available at dealer) | NA | O | O | O |
| Auxiliary Camera Prep, includes vehicle trailer wiring, camera  display in radio, 12-pin connector at rear frame rail | NA | O/P | O/P | O/P |
| Surround View camera (five digital cameras) | NA | P | P | P |

#### Parking Sensors

| Parking Sensors | TRADESMAN | SLT | LARAMIE | LIMITED |
| --- | --- | --- | --- | --- |
| Rear park assist | O | O | O | S |
| Front/rear park assist | O | O | O | S |

#### Safety Features

| Safety Features | TRADESMAN | SLT | LARAMIE | LIMITED |
| --- | --- | --- | --- | --- |
| Security alarm | NA | O | S | S |
| Backup alarm (audible alarm when vehicle is in reverse) | O | O | O | O |
| Lane Departure Warning, (Lane Keep Assist) | P | P | P | P |
| Adaptive Steering (standalone option) | P | P | P/O | P/O |
| Adaptive Cruise Control with Stop | P | P | P | P |
| Ready Alert Braking | S | S | S | S |
| Full-speed Forward Collision Warning-Plus (available with Adaptive Cruise) | P | P | P | P |
| Lane Keep Assist | P | P | P | P |
| Adaptive Steering | P | P | P | P |
| Tire-fill alert system (must have 5-in. radio with Tradesman) | O | O | S | S |
| Selectable tire fill alert (packaged with 8.4-in. and 12-in. radios on SLT) | NA | P | S | S |
| Tire-pressure Information System | O | S | S | S |
| Tire-pressure Monitoring Display | S | S | S | S |
| Trailer Tire-pressure Monitoring | NA | O | O | O |
| Trailer Reverse Guidance | NA | P | P | P |
| DOT– certified Roadside Safety Kit (DOT fire extinguisher,  three reflecting triangles, spare fuses, two red vinyl flags) | O | O | O | O |
| Max speed settings (65 mph, 70 mph, 77 mph) | O | O | O | O |
| Auto high beam headlamp control | P | P | P | S |
| Rain Sensing Wipers | P | P | P | S |
| Auxiliary Reverse Lamps (packaged with SLT) | O | O/P | S | S |

### EQUIPMENT PACKAGES

| EQUIPMENT PACKAGES | TRADESMAN | SLT | LARAMIE | LIMITED |
| --- | --- | --- | --- | --- |
| **Electrical Accessory Group**  220-amp alternator  Voltage Monitoring Auto Idle Up  Trailer Brake Control | O | O | O | O |
| **Ambulance Prep Group**  220-amp alternator  Voltage Monitoring Auto Idle Up  Remote rear heat/AC (provides ability to run auxiliary mounted heater and  A/C independently of instrument panel controls)  A/C line tap and engine coolant access for upfitter  Foam roof blocks (included with Regular Cab only) | O | O | O | O |
| **Chrome Appearance Group**  Chrome front bumper (3500/4500/5500)  Chrome grille (3500/4500/5500)  Chrome inserts  Chrome clad steel wheel on 3500 DRW  Chrome clad steel wheel on 3500 SRW  New bright wheel cover (4500/5500) | O | NA | NA | NA |
| **Cold Weather Group (Diesel option)**  Engine block heater cord  Winter front grille cover | O | O | O | O |
| **Comfort Group**  Heated steering wheel  Leather-wrapped steering wheel and audio controls  Cluster 3.5-in. TFT color display | NA | O | NA | NA |
| **Tradesman Level 1 Equipment Group**  Overhead console (Regular Cab)  Power windows (Regular Cab)  Power door locks (Regular Cab) (speed sensitive actuation)  Power black trailer tow mirrors (Regular Cab)  Door trim: (Regular Cab)  (wrapped bolster/armrest, 360 door handles, join seam, Iron Gray painted surround and accent)  Remote Keyless Entry  Interior door handles, satin chrome polished | O | NA | NA | NA |
| **Laramie Level 1 Equipment Group**  Auto high beam headlamp control  Rain-sensing wipers  Foam bottle door inserts  Ventilated three-level front driver/passenger seats  Power-adjustable pedals  Radio, driver, seat, mirror, pedals memory  CD player | NA | NA | O | NA |
| **Laramie Level 2 Equipment Group  (Includes Laramie Level 1 Equipment Group Content)**  Uconnect 8.4 (AM/FM/SAT/Bluetooth/NAV/Voice)  17 speakers  Wireless charging pad  Rear seat heat (three level) | NA | NA | O | NA |
| **Limited Level 1 Equipment Group**  12-in. radio  17-speaker system  Full-speed Forward Collision Warning Plus with Auto Emergency Braking  Adaptive Cruise Control with Stop  Surround View Camera | NA | NA | NA | O |
| **Premium Lighting Group**  LED headlamps  LED fog lamps  Cluster 3.5-in. TFT color display | NA | O | NA | NA |
| **Safety Group**  Forward Collision Warning Plus with Auto Emergency Braking  Adaptive Cruise Control with Stop, Go and Hold  Lane Keep Assist  Adaptive steering  Rain-sensing wipers  Smart Beam  Trailer Brake Control (Packaged with Tradesman and SLT) | O | O | O | O |
| **Tow Technology Group**  Surround View camera  Trailer reverse guidance  Auxiliary reverse lamps, mirror-mounted  Power convex mirrors | NA | O | O | O |
| **Heavy-Duty Snowplow Prep Group**  220-amp alternator  Transfer case skid plate  Heavy Duty Front Suspension Group (4500 and 5500) | O | O | O | O |
| **Luxury Group**  Passenger/driver cloth visors with incandescent illuminated mirrors  Universal garage door opener  Rear dome lamp with on/off switch  Cluster 7.0-in. TFT color display  Leather-wrapped steering wheel with remote audio control buttons  Rear backlight, power sliding (Crew Cab only)  Foam bottle door insert  115-volt outlet (front)  115-volt outlet (rear) (Crew only)  Upper and lower glove box lighting  Power adjustable pedals  Rear: dual remote USB port (Crew only) 2 A/C pairs; one pair fully functional, one pair charge only  Upper glove box door with SLT badge | NA | O | NA | NA |
| **Max Tow Package (Requires Diesel and Aisin)**  12-in. rear axle (3500)  4.10 axle (3500)  4.44 axle (4500)  4.89 axle (5500)  6.7-liter  Aisin transmission  Trailer brake controller | O | O | O | O |
| **Max Payload Package (6.4-liter 5500 only)**  19,000-lb. GVWR  19,500-lb. GVWR  4.89 axle ratio | O | O | O | O |
| **Rollback Carrier Group**  Voltage monitoring auto idle up system  Rollback carrier adaptation brackets  220-amp alternator  Left- or right-side PTO  22-gallon mid-ship gas tank | O | O | NA | NA |
| **Rear Interior Trim Delete Group (Regular Cab only)**  Delete front center seat  Delete rear floor storage tray  Delete cab back trim panel | O | O | NA | NA |
| **15,000-lb. GVWR Package**  Includes 15,000-lb. Gross Vehicle Weight Rating (4500)  4x2, 4x4 | O | O | O | O |
| **16,000 GVWR Package**  Includes 16,000-lb. Gross Vehicle Weight Rating (4500)  4x2, 4x4 | O | O | O | O |

###