# 2023 Jeep® Wrangler 4xe

## FEATURE AVAILABILITY

S = Standard. O = Optional. P = Part of package. NA = Not available.   
Note: some features and/or applications may be late availability.

### ENGINE / TRANSMISSION

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | Wrangler (four-door) | Wrangler (four-door) |
| ENGINE | TRANSMISSION | Sahara 4xe | Rubicon 4xe |
| 2.0-liter Inline four-cylinder with eTorque belt-start generator/motor and integrated transmission traction motor | Eight-speed automatic | S | S |

### MECHANICAL / CAPABILITY

|  | Wrangler (four-door) | Wrangler (four-door) |
| --- | --- | --- |
| MECHANICAL / CAPABILITY | Sahara 4xe | Rubicon 4xe |
| Axle Ratios |  |  |
| 3.73:1 (EcoDiesel only for Sport, Sport S and Sahara) | S | NA |
| 4.10:1 | NA | S |
| Axles |  |  |
| 3rd generation Dana 44 heavy-duty solid front | S | S |
| 3rd generation Dana 44 heavy-duty solid rear | S | S |
| Differentials |  |  |
| Trac-Lok limited-slip, rear | O | NA |
| Tru-Lok front and rear, electronic remote locking | NA | S |
| Sway Bar Disconnect — electronically controlled, front | NA | S |
| Towing — Trailer-tow Group includes Class II hitch receiver, four-pin and seven-pin adapter, 240-amp alternator, 700-amp battery, auxiliary switches | O | O |
| Trailer-sway control | S | S |
| Transfer Case |  |  |
| Selec-Trac full-time transfer case (2.72:1) | S | NA |
| Rock-Trac NV241 OR, full-time, shift-on-the-fly transfer case; 4:1 low-gear ratio | NA | S |

### EXTERIOR

|  | Wrangler (four-door) | Wrangler (four-door) |
| --- | --- | --- |
| EXTERIOR | Sahara 4xe | Rubicon 4xe |
| Doors |  |  |
| Full metal doors with power windows | S | S |
| Half doors | P | P |
| Door Locks |  |  |
| Power door locks (speed-sensitive locking) — door-mounted switches | S | S |
| Fender Flares |  |  |
| Two piece — body-color | S | O |
| Two piece — Rubicon | NA | S |
| Forward-facing off-road camera | O | O |
| Glass |  |  |
| Deep-tinted sunscreen rear and quarter windows | S | S |
| Corning Gorilla Glass windshield | O | O |
| Power windows (front and rear), driver and pass one-touch down | S | S |
| Grille |  |  |
| Body-color grille — Sahara accent throats and headlamp rings | S | NA |
| Body-color grille — Rubicon accent throats and headlamp rings | NA | S |
| Lighting |  |  |
| LED reflector headlamps (packaged with LED Lighting Group) | S | S |
| LED fog lamps (packaged with LED Lighting Group) | S | S |
| Automatic headlamps | S | S |
| Mirrors |  |  |
| Mold-in color manual folding mirrors | S | S |
| Power-heated mirrors | S | S |
| Blind-spot indicator in mirror | P | P |
| Side steps — tubular, diamond plate surface pattern | O | NA |
| Skid plates — fuel tank and transfer case | S | S |
| Rock rails — black, painted steel, heavy-duty, protective | NA | S |
| Tires |  |  |
| All-terrain tires, 285/70R17 BF Goodrich KO2, BSW, Off-road | NA | S |
| All-season tires, 275/55R20 Bridgestone Dueler H/L Alenza | S | NA |
| Tops |  |  |
| Sunrider folding soft top with sunroof feature | S | S |
| Premium Sunrider soft top | O | O |
| Freedom Top three-piece modular hardtop with rear wiper/washer, rear defroster, full-framed doors and Freedom Panel storage bag | O | O |
| Body-color three-piece hardtop | O | O |
| Powertop | O | O |
| Dual Top Group (available premium Sunrider) | O | O |
| Mopar Sunrider flip top for hard top | O | O |
| Tow hooks — two front, one rear | S | S |
| Wheels |  |  |
| 17-in. aluminum Rubicon machined / painted black | NA | S |
| 20-in. aluminum fully painted black | S | NA |

### INTERIOR

|  | Wrangler (four-door) | Wrangler (four-door) |
| --- | --- | --- |
| INTERIOR | Sahara 4xe | Rubicon 4xe |
| Air Conditioning |  |  |
| Air conditioning with automatic temperature control — dual zone | S | S |
| Cabin air filter – dual zone | S | S |
| Console — full-floor with front and rear cup holders, locking storage and armrest | S | S |
| Floor heat ducts — rear | S | S |
| Floor Mats |  |  |
| Front and rear | S | S |
| Rear cargo mat | P | P |
| Mopar slush mats | O | O |
| Lighting |  |  |
| LED front cup holder | S | S |
| LED rear cup holder | S | S |
| LED overhead courtesy lamp | S | S |
| LED second-row overhead / cargo courtesy lamp | S | S |
| LED door bezel ambient lamp | S | S |
| LED foot well courtesy — functional | S | S |
| LED ambient footwell lamp — mood/accent light | S | S |
| LED center console ambient lamp | S | S |
| Passive entry | S | S |
| Push-button start | S | S |
| Remote keyless entry with mechanical flip key | S | S |
| Remote start system | O/P | O/P |
| Seating |  |  |
| Premium cloth seats | NA | S |
| Premium McKinley trimmed seats | S | NA |
| Leather-trimmed seats | NA | O |
| Heated front seat | P | P |
| Driver seat — six-way manual (fore/aft, recline, height adjust) | S | S |
| Front passenger seat — four-way manual (fore/aft, recline) | S | S |
| Two-way lumbar (driver only) | S | S |
| Tilt/telescoping steering column — manual | S | S |
| Steering Wheel |  |  |
| Premium Wrapped | S | S |
| Mounted audio controls | S | S |
| Electronic Vehicle Information Center (EVIC) controls | S | S |
| Heated steering wheel | P | P |
| Speed and cruise control | S | S |
| Universal garage door opener | S | S |
| Hardtop headliner | O | O |
| Wash-out interior with removable carpet and drain plugs | S | S |

### UCONNECT / MULTIMEDIA

|  | Wrangler (four-door) | Wrangler (four-door) |
| --- | --- | --- |
| UCONNECT / MULTIMEDIA | Sahara 4xe | Rubicon 4xe |
| Audio System |  |  |
| Nine Alpine speakers with all-weather subwoofer and 552-watt amplifier | S | S |
| Auxiliary power, 115-volt outlet in center console | S | S |
| Media hub (one full-function USB and auxiliary port) | S | S |
| Power outlet, 12-volt, instrument panel | S | S |
| Power outlet, 12-volt, cargo area | S | S |
| Radio with Uconnect 4C NAV with 8.4-in. display | S | S |
| SiriusXM Radio — includes six-month trial subscription | S | S |
| SiriusXM Guardian Connected Services — includes one-year trial subscription | S | S |
| SiriusXM Travel Link — includes five-year trial subscription | S | S |
| SiriusXM Traffic Plus — includes five-year trial subscription | S | S |
| Uconnect Voice Command — hands-free calling with address book and Bluetooth | S | S |
| USB — fully functional in center console | S | S |
| USBs — two charge-only in the back of the center console | S | S |

### SAFETY & SECURITY

|  | Wrangler (four-door) | Wrangler (four-door) |
| --- | --- | --- |
| SAFETY & SECURITY | Sahara 4xe | Rubicon 4xe |
| Advanced multistage front airbags | S | S |
| Supplemental front seat side airbag | S | S |
| Front passenger seat Occupant Detection System | S | S |
| Driver and front passenger seat belt alert (all markets) | S | S |
| Rear Child Seat Anchors — LATCH | S | S |
| Tire-pressure Monitoring | S | S |
| Blind-spot Monitoring | P | P |
| Rear Park Assist | P | P |
| Rear backup camera with dynamic gridlines | S | S |
| Sentry Key antitheft engine immobilizer | S | S |
| Vehicle theft alarm — protects doors and liftgate | S | S |
| Antilock braking system with hydraulic assist braking | S | S |
| Electronic Roll Mitigation | S | S |
| Electronic stability control — includes hydraulic assist brake booster and traction control | S | S |
| Hill-descent Control (packaged with eight-speed automatic transmission) | S | S |
| Hill-start Assist | S | S |

### PACKAGES / EQUIPMENT GROUPS

|  | Wrangler (four-door) | Wrangler (four-door) |
| --- | --- | --- |
| PACKAGES / EQUIPMENT GROUPS | Sahara 4xe | Rubicon 4xe |
| **Jeep Active Safety Group** — includes ParkSense rear park assist, Blind-spot Monitoring and LED taillamps | O | O |
| **Jeep Advanced Safety Group** — includes adaptive cruise control, forward collision warning | O | O |
| **Infotainment Group** — includes 8.4-in. radio with NAV, inside electrochromatic rearview mirror, SOS call located on the header above rearview mirror and nine-speaker premium audio system with all-weather subwoofer | S | S |
| **Cold Weather Group** — includes heated front seats and heated steering wheel remote start | O | O |
| **Trail Rail Cargo Management Group** — includes load floor, four anchor pods, swing gate rail and rear cargo mat | O | O |
| **Black Three-piece Hardtop Group** — includes black three-piece hardtop, rear window defroster and rear window washer and wiper | O | O |
| **Body-color Three-piece Hardtop Group** — includes color three-piece hardtop, rear window defroster and rear window washer and wiper | O | O |
| **LED Lighting Group** — includes LED headlamps with round signature lighting, LED front fog lamps, LED daytime running lamps, LED Park Turn and LED taillamps | S | S |
| **Trailer-tow and Heavy Duty Electrical Group** — includes four auxiliary switches, heavy-duty 240-amp alternator, trailer tow, Class II hitch receiver, four-pin and seven-pin adapters | O | O |
| **Rubicon heavy-metal winch-capable bumpers** — includes front and rear steel bumpers | NA | O |

###